Divide excavation area into 10m x 10m grid squares with a means to identify the grid on site

**START**

Identify method, Treat and

Re-test

Yes

Do   
samples have   
hazardous properties or substances?

**WM3 Appendix B & C**

Take one sample from each grid square at each 1m depth of planned excavation

Can treatment remove or reduce hazards?

Yes

Send samples for **Composition / Characterisation** testing

No

Are   
hazardous   
properties acceptable at

La Collette?

**Check Non-Inert**

**WAC Table 2**

No

Hazardous: assign EWC code (**WM3 Appendix A**) and carry out **leach** testing

Yes

Non-hazardous: assign EWC code (**WM3 Appendix A**) and carry out **leach** testing

No

Are leach results within La Collette hazardous limits? **Check Non-Inert WAC Table 2**

No

Are leach results within La Collette inert limits?

**Check Inert WAC**

**Table 2**

Yes

No

Are leach results within La Collette SNRC limits?

**Check Inert WAC**

**Table 2**

No

Yes

**END**

**Dispose as Stable Non-Reactive Contaminated**

Yes